**High Speed Low Flying Targets (HSLFT)**

1. **Brief Description/ Technical Details.**

(a) High speed low flying Aerial target

(b) Expendable in nature and launched from ship upto Sea State 3

(c) Speed greater than or equal to 350 Knots

(d) Endurance greater than or equal to 30 min at max speed and 40 min at Economical speed

(e) Flight Altitude 5m to 6000m

(f) Pre-programmed autonomous flight using way point navigation

(g) Target should be capable of being controlled upto 75 Km based on clear Line of sight

2. **Quantity.** 150

3. **Tentative Timelines for Development/Production**. Two- three years